BGSF111

1378´ 860´

1411´

2000´

/

2067´

1

0

0

0

1

0

0

0

1

0

0

0

1

0

00

1

0

0

0

1

0

0

0

1

0

0

0

1

0

00

1

0

0

0

1

0

0

0

1

0

0

0

1

0

0

0

2

0

0

0

2

0

0

0

1

0

0

0

1

0

0

0

1

0

0

0

Procedure in airspace

2

0

00

2000 classified G.

hdg

D2.5 ISF D3.5 ISF D4.5 ISF

D10.0

D15.0_{ISF}

D17.0_{ISF}

Hazard Beacon

382 SF

100´ 5.2

NDB

165´

Apt. Elev

11-1

·· ··· ··-·

LOC DME

282°

Gnd speed-Kts 70 90 100 120 140 160

CHANGES:

MSA

MISSED APPROACH:

0 5 5 10 15

1 in=5 NM

JEPPESEN

SF NDB

LOC 109.55 ISF

5300´

(3900´) (4300´)

A B C D

CIRCLE-TO-LAND

STRAIGHT-IN LANDING RWY

ALS out

10

Alt Set: hPa & IN Trans level: By ATC Trans alt: 7000´ (6900´)

MKR

··· ··-·

102° 109.55 ISF

CAUTION: Adhere strictly to the prescribed procedure due to high surrounding terrain. Expect moderate turbulence on final approach with winds in excess of 20 KT.

ALTITUDE (HAT)

ISF LOC DME 9.0 7.0 6.0 5.0 4.0 3.0

2750´(2650´) 2050´(1950´) 1700´(1600´) 1350´(1250´) 1000´ (900´) 650´ (550´)

ISF

117°

CAT C & D

CAT A & B

306°

294°

MAP at D2.5 ISF

MDA(H) 450´ (350´)

Descent Gradient 5.8% 411 529 587 705 822 940

PANS OPS

RWY 10

Start turn at

3 Min

2^1 2 Min

5300´ 3300´

3100´ 1200´ 750´ D10.0_{ISF} ISF ISF ISF

(5200´)

(3200´)

(3000´)

(1100´) (650´)

(350´)

OCA(H) RWY 10 450´

D2.5

1.0 3.2

66-50

67-00

51-20 51-10 51-00 50-50 50-40 50-30

GREENLAND

4400

MKRLOCDMERwy10

CAT C & D

A & B

306° 294°

102°

102°

126.2_{MISSED APCH CLIMB GRAD MIM 5.0%}

Missed apch climb gradient mim 5.0% outbound leg of holding to 2 Min

to intercept LOC at 3300´ (3200´).

A & B:

C & D:

C & D

A & B

D17.0

D15.0_{7.0}

CAT A & B: 5.0

SONDRE STROMFJORD,

SONDRE STROMFJORD

PROCEDURE AFTER HOLDING: Extend

(CAT A & B 3 Min), then turn LEFT

Rwy Elev: 4 hPa

Max Kts 100 135 180 205

Not authorized North of airport

1500´ 1900´ 2500´

2800´

(1335´) (1735´)

(2335´)

(2635´)

2000m 2400m

4800m

4800m

MDA(H)

SONDRE STROMFJORD

From D25.0 the LOC is not to be used outside 5° north and 15° south of LOC-course. From D17.0 the LOC is not to be used outside 10° north of and 15° south of the LOC-course.

D4.5

D3.5

2.3 1.0 0.9

© JEPPESEN SANDERSON, INC., 1992, 1995. ALL RIGHTS RESERVED.

2000m

1200m VIS 1600m

1500m RVR

, then immediately turn RIGHT on heading 117° climbing to 4000´ to 4400´ and join holding.

, then turn RIGHT to NDB climbing

· ··· · 12

ISF ISF Climb AHEAD until reaching MKR^0

1083´

1378´

1510´ 1871´

1542´

1871´

1493´

1936´

2067´

1772´

2034´

2170´

2300´

17 NOV 95

118.3

*SONDRESTROM Approach (R)

*SONDRESTROM Tower

Contour depiction.