BIRKAPT

NOT APPLICABLE

02_{015°}

25_{245°}

14_{136°}

32_{316°}

Elev Var 20°W

REYKJAVIK

BIRK11-1 JEPPESEN

CHANGES:

RWY

ADDITIONAL RUNWAY INFORMATION

Threshold

LANDING BEYOND

USABLE LENGTHS

WIDTH

TAKE-OFF

Glide Slope

20_{195°}

3150´

960m

07_{065°}

Elev

Elev

Elev

Elev

Elev

Elev

187´

369´

282´

233´

100´

165´

141´

4767´

5738´1749m

1453m

18´

20´

38´

38´

26´

Flashing Runway Alignment Beacon

Buildings up to 130´

H21-37

H9 H2 H6

H3 H13 H14 H11

H4

H1 H7

F

A

ARP E

H1 Hangar 1

LEGEND 29´

Control Tower

137´

REYKJAVIK, ICELAND

REYKJAVIK Ground 121.7

02 20 45m

RL 30m

All Rwys

TAKE-OFF AIR CARRIER (FAR 121)

A B C D

AIR CARRIER

Adequate Vis Ref 2 Eng 3 & 4 Eng

HIRL

250m 300m 500m

400m 400m RVR RVR RVR VIS

64-07

64-08

64-07

64-08

21-59 21-58 21-57 21-56 21-55 21-54

21-59 21-58 21-57 21-56 21-55 21-54

VOT 113.0

Flashing runway alignment beacon.

HIRL VASI HIRL HIALS VASI

Portable RL O/R

RL PAPI-L (angle 3.0°)

PAPI-L (angle 3.0°)

07 25 14 32

4879´

4364´_{1330m} _{5305´ 1617m}

148´ 98´ 148´ 45m 1273m 4177´

3081´ 939m

856m

2808´

5305´ 1617m

1487m RVR

For acft requiring only LCN 20: For acft requiring only LCN 20:

5312´(1619m). 5738´(1749m).

Take-off Rwy 07 is not permitted unless

crosswind component on other Rwys exceeds 10 knots.

282´

45´

Rwys 07/25, 14/32

Rwy 02/20

Tower 118.0

*ATIS 128.1

084.0°/19.7 From KEF 112.0

© JEPPESEN SANDERSON, INC., 1991, 1999. ALL RIGHTS RESERVED.

Lctr Flashing Runway Alignment Beacon G

151´

141´

5000

1500

1000

1000 500 0 0 Feet

Meters

2000 3000 4000

N64 07.7 W021 56.6

105´

22 NOV 96

Minimums.